
Step 1:


第三方机器或者本地机器

Create Certificate in Power shell

$cert = New-SelfSignedCertificate -DnsName "CN=PreactorIntegrationTest2,T=SimaticIT UA Foundation" -CertStoreLocation "cert:\LocalMachine\My"-KeyExportPolicy Exportable -KeySpec Signature



Execute without any error




红色名字部分，可以自定义


Step 2


第三方机器或者本地机器

One MMC (Run –MMC)


File Add/Remove Snap in









Click ok



View Certificate





Locate the certificate created under Intermediate Certificate Authorities





Step 2 : Export certificate as .CER file

On Preactor Machine open MMC and locate certificate as shown in previous step , right click on the certificate and export













Browse the path and specify the file name












Step 3 : Install certificate on Preactor Application Machine


Locate the .CER file created and double click on it





Click on Install Certificate












Step 4 : Install certificate in UADM server Machine from the .CER File

Copy the .CER file generated on 第三方机器或者Studio机器上in the previous step and paste in UADM server machine



Double click on the .CER file



Click on Install certificate

